# Procedure

1. The Windows Operating System version of X-Plane 10 was loaded in the AE department flight simulator.
2. X-Plane was set up to record flight data to an external text file.
3. The Kingair aircraft was selected and loaded.
4. The Kingair was flown to 5,000 feet and trimmed.
5. The three dynamic maneuvers were executed. Time data for each maneuver was recorded.